Cross reference with the standard pottery

Ratio of standard pottery to sample should be the same

Identify as much as fast as possible

K40 got lost in the background

Do more sources for efficiency calibration