* To find Bromine in 1110C sample spectra
  + A = N \* flux \* cross section \* exp^(blah) = cps/g / (branching ratio \* efficiency)
  + Use reported flux
  + Calculate the flux from the pottery
* If there is no peak, take ROI of region and report # counts <= sqrt(Gross counts)